Name………………………………………..ADM No……………. Class………………..

**448/2**

**ELECTRICITY**

**MARKING SCHEME**

**Paper 2**

**AUGUST-SEPTEMBER 2022**

**Time: 2 ½ hours**

**MECS CLUSTER JOINT EXAMINATION**

**FORM FOUR END YEAR EXAMINATION 2022**

**ELECTRICITY**

**Instructions To Candidates**

*1. There are* ***FIVE*** *exercises in this paper*

*2. Candidates are allowed* ***30 minutes*** *for each exercise*

*3. Each exercise will be awarded a maximum of* ***20 marks***

*4. Write your* ***Name*** *and* ***Index number*** *at the top of this page*

*5. Do NOT do work related to other stations while at a different station*

*6. Attempt* ***All*** *the exercises as directed by the examiner(s)*

*7. All dimensions are in* ***millimeters*** *unless it’s indicated otherwise*

**For Examiner’s Use Only**


|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Exercise** | **1** | **2** | **3** | **4** | **5** | **Total** |
| **Total Marks** |  |  |  |  |  |  |
| **Marks Scored** |  |  |  |  |  |  |
| **Grand Total** | | | | | |  |

*This paper consists of* ***8 printed pages****. Candidates should confirm that all the pages are printed as indicated and that no questions are missing.*

**MARKING SCHEME**

**EXERCISE 1**

1. Figure 1 shows an electrical circuit.



*Figure 1*

1. Using the components, materials and equipment provided. Connect the circuit as shown in Figure 1 on the breadboard.

**Let the examiner check your work.** (6 marks)

1. With S1 **ON**, measure and record the total current IT.

IT=……***200***…………………………………. mA (1 mark)

1. Measure and record the currents.

I1=……***127***…………………………………. (mA)

I2=……***73***…………………………………. (mA)

I3=……***73***…………………………………. (mA)

1. (i) In the circuit, replace R3 with R4.

**Let the examiner check your work.** (2 marks)

(ii) Repeat steps (a) to (c). (4 marks)

IT=……***175***…………………………………. (mA)

I1=……***102***…………………………………. (mA)

I2=……***63***…………………………………. (mA)

I3=……***63***…………………………………. (mA)


1. (i) Explain the relationship between currents I2 and I3 (2 marks)


***magnitude is the same since its flowing through the same branch***

(ii) State the effect on the current IT when R3 is replaced with R4. (2 marks)

**EXERCISE 2**

1. Using the tools, equipment and materials provided, fabricate the bracket shown in **Figure 2.** (20 marks)





*Figure 2*


**EXERCISE 3**

1. Using the tools, materials and equipment provided, carry out the following tasks.
2. Terminate the three heat resistant flexible cable to the top plug and the iron box. (15 marks)
3. Turn the thermostat switch ‘**ON’** at the maximum position. (1 mark)
4. Measure and record the values of Resistance of the element in **Table 1**. (4 marks)

|  |  |
| --- | --- |
| **TEST BETWEEN** | **READINGS OBTAINED** |
| 1. Live and Neutral at plug | **HIGH** |
| 1. Live and Earth at Plug | **HIGH** |
| 1. Earth at Plug and Iron box body | **ZERO** |
| 1. Neutral at Plug and Iron box | **LOW** |

**EXERCISE 4**

1. **Figure 3** shows the block diagram of an electronic circuit marked R.



*Figure 3*

Use the equipment and accessories provide to perform the following tasks;

1. Set the power supply voltage to 10V output.
2. With the power supply off and switch S off, connect the equipment to the terminals of circuit **R** at points (+) and (-) as shown.
3. A and B as an Ohmmeter
4. X and Y an ammeter
5. S and T to power supply.

**Let the examiner check your work.** (3 marks)

1. Turn the power supply **ON** and turn the switch **ON**.

Adjust the potentiometer to obtain RL values as shown in Table 2.

1. In each case, measure and record in table 2 the corresponding values of circuit current I and calculate values of circuit power in Watts.

|  |  |  |
| --- | --- | --- |
| RL(kΩ) | I(A) | P(W) |
| 0 | ***0*** | ***0*** |
| 5 | ***0.19*** | ***0.181W*** |
| 10 | ***0.173*** | ***0.299W*** |
| 15 | ***0.16*** | ***0.384W*** |
| 20 | ***0.153*** | ***0.468W*** |
| 25 | ***0.147*** | ***0.540W*** |
| 30 | ***0.14*** | ***0.48W*** |
| 40 | ***0.131*** | ***0.473W*** |
| 60 | ***0.11*** | ***0.47W*** |
| 80 | ***0.1*** | ***0.387W*** |
| 100 | ***0.09*** | ***0.364W*** |


(11 marks)

1. Plot a graph of power against load resistance on the graph provided on the last page. (4 marks)
2. Determine the value of load resistance that allows maximum power transfer from the graph provided in 4(e). (2 marks)



**EXERCISE 5**

1. Figure 4 shows the layout of a lighting final circuit.



*Figure 4*

Using PVC sheathed cable, install the circuit such that the lamp is controlled from one point. (20 marks)