**NAME: --------------------------------------------------------------- ADM NO. ------------------------**

**CLASS ---------------------------------------------------------------- DATE: ---------------------------**

**HOMESCIENCE (CLOTHING CONSTRUCTION)**

**441/2**

**PRACTICAL**

**AUG/SEP 2022**

**TIME 2 ½ HRS**

**MINCKS GROUP OF SCHOOLS**

**FORM FOUR**

**PAPER 2**

**TERM 2 2022**

A pattern of a girl’s dress is provided. You are advised to study the sketches instructions and layout carefully before you begin the test.

***Materials provided.***

1. Pattern pieces
2. Bodice front
3. Bodice back
4. Skirt front
5. Skirt back
6. Sleeve
7. Collar

G. Cut out a crossway strip measuring 18cm long by 4cm wide.

2. Plain light weight fabric 70cm long by 90cm wide.

3. Cotton sewing thread to match the fabric.

**THE TEST**

Using the materials provided cut out and make the left side of the girl’s dress to show the following processes

1. Making of the dart at the front bodice. (6 mks)
2. Making of a shoulder seam using a double stitched seam. (8 mks)
3. Making of the side seam on bodice and skirt using an open seam. (13 mks)
4. Attaching of the bodice pieces to the skirt pieces using a plain seam and neatening half of the back using loop stitches. (10 mks)
5. Preparation of the collar. (4 mks)
6. Attaching of the collar using a crossway strip.. (13 mks)
7. Making of an under arm seam using an open seam. (6 mks
8. Preparation and attachment of the sleeve. Do not trim or neaten the seam allowance. (8 ½ mks)

**OMIT**

The management of the lower hem of the skirt and the sleeve