**Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Index.No \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**MARKING SCHEME 441/2**

**HOME SCIENCE**

**ARISE AND SHINE TRIAL1 EXAMINATION**

**AUGUST/SEPTEMBER 2022**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **SNR****NO** | **AREAS OF ASSESSMENTS** | **MAX** **SCORE** | **ACTUAL** **SCORE** | **REMARKS** |
| 1 | **PRESENTATION**(a). work well pressed(1) and folded(1/2 )(b). Label (½ )firmly fixed(1) on single (1/2)fabric without concealing details (1/2)(c). pins ½ needles (1/2) taking threads and unnecessary threads(½ ) removed(d). made up for the LEFT HALF (1) | 11/2 2½ 1½ 1 |  |  |
|  | **Sub total** | 6½  |  |  |
| 2 | **Cutting out**(a). All five pieces (5 x ½).(b). Smooth cutting of skirt CF (1)(c). Smooth cutting of skirt CB(1)(d). Smooth cutting of bodice back (1) and on straight grain (1) to within 3mm.(e). Sleeve cut on straight grain (1)(f). Smooth cutting of back neck facing (½) and on straight grain (½) to within 2mm.(g). Smooth cutting of skirt lower edge(1) | 2½ 1 1 2111 |  |  |
|  | **Sub total** | 9½  |  |  |
| 3 | **SHOULDER SEAM (OPEN SEAM)**(if not open seam award zero)(a). Seam joined with straight stitchery (1)(b). Well neatened raw edges (1X2)(c). Evenness of seam allowance. (2)(d). seam pressed open (½ X 2) and flat R.S (½ X2), WS(½ X2) at the neckline and at the arm hole (e). Correct size of seam allowance 1cm to within 2mm (0.8cm – 1.2cm) (½ x 1) | 12231 |  |  |
|  | **Sub total** | 09 |  |  |
| 4 | **NECK FACING**(a). Back and extended front facing joined with straight stitchery (1/2) seam trimmed (1/2 ) pressed open(1/2) andunneatened (1/2)(b). Facing attached to neckline with smooth stitchery (1)(c). Seam trimmed (1) snipped (2) and under stitched (2)(d). Facing seam and shoulder seam meeting to within 2mm (2) at neckline and shoulder seam (2) and held down with a (1) stitch.(e). Centre front of extended facing well pointed (1)(f). Extended facing well folded (1/2) and flat (1/2) at the centre front.(g). Flatness of neck facing (front and back) (2) | 2155112 |  |  |
|  | **Sub total**  | 17 |  |  |
| 5 | **FRENCH SEAM**(if not French seam award zero) from B - H(a). Underarm seam and side seam made before (1) sleeve is attached.(b). Straight stitchery of seam (1x2)2(c).Seam well-trimmed (1/2) X2, no threads on RS (1/2X2)2(d). Seam well knife edged (½ X2)1(e). Evenness of seam (1/2 X2)1(f). Correct size (6mm) to within (4mm-8mm)(½ X2)1(g). Seam pressed towards the back at armhole(1/2X2) and at waist line (1/2 X2)(h). Flatness of seam at armhole and at 2 the waistline (½ x 2).(i). Side seam and underarm seam meeting at (1) within 2mm. | 12211121 |  |  |
|  | **Sub total** | 13  |  |  |
| 6 | **SLEEVE**(a). Good hang (b). Easing evenly distributed (1) around the crown.(1)(c). Armhole seam made with smooth stitchery(d). Correct positioning of sleeve i.e back to back (1) bodice and front on front bodice (1)(e). Armhole seam smoothly trimmed (1 cm) (1)(f). Attached at side seam to within 2mm meeting point and round allowance (0.8 – 1.2cm) (½ x2)(g). A quarter of the armhole seam neatened with loop stitches (1) using single thread (½) sleeve hem managed by edge-stitching (1) and turned (1) and held down with tacking (1) stitch. Only using single thread (½) sleeve hem size (1.2cm to within 2mm (1cm to 1.4cm) 1 | 12122151 |  |  |
|  | **Sub total** | 15  |  |  |
| 7 | **(b) NEATENING THE ARMHOLE**(If not loop stitches award zero)(i). Loop stitches evenly spaced (1) and even in length (1)(b). Stitches securely fastened on (½) and off (½) | 21 |  |  |
|  | **Sub total** | 3 |  |  |
| 8 | **SKIRT**(a). Gathers well distributed (2) and good hang (2)(b). Smooth (1) stitchery (1) of the waistline seam.(2)(c). Evenness of seam. (1)(d). The space at the extended facing part of the waistline seam not gathered. (1)(e). Stitching line between the two gathering rows (1) (f). Award marks if gathers are of good quality. (1) | 2221 111 |  |  |
|  | **Sub total** | 10 |  |  |
| 9 | **FACING**(a). Free edge facing smoothly neatened.(b). Facing pressed flat. | 11 |  |  |
|  | **Sub total** | 2 |  |  |
| 10 | IMPRESSION [Neatness / quality of work]. **Sub total** | **5** |  |  |
|  | **GRAND TOTAL ÷ 2** | **90** **2 = 45** |  |  |