**MARKING SCHEME 441/2**

**HOME SCIENCE**

**CLOTHING AND TEXTILE**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S,NO** | **AREAS OF ASSESSMENT** | **MAX** **SCORE** | **ACTUAL** **SCORE** | **REMARKS** |
| 1(a)(b)(c)(d) | **PRESENTATION**Work well pressed and foldedLabel (1) firmly fixed (11/2 ) without concealing details(1) and on single (1) fabricPins needles (1 ½ ) and tacking threads and Unnecessary threads removed.(1)Left half made 1 ½  | 2 ½ 2 ½ 21 ½ 11 ½  |  |  |
|  | **Sub total** | 11 marks |  |  |
| 2(a)(b)(c)(d)(e) | **CUTTING OUT**-All pieces cut out 5 interfacing(5)- Blouses front cut smoothly (1/2) and on a straight grain- Blouse back cut smoothly ½ and on straight grain (1 ½ )- Pocket cut smoothly and on straight grain (1 ½ )- Collar cut smoothly (1/2) and on straight grain (1 1/2) | 5½ ½ 1½ 1 ½  |  |  |
|  | **Sub total** | 10 marks |  |  |
| 3 | **DOUBLE STITCHED SEAM SHOULDER**If not double stitched seam award ‘O’(a). seam made on R.S (1/2) (b). Straight stitchery (1) on shoulder line(c). Raw edges well tucked under ½ (d). 2nd row of stitchery don close to the fold ½ and straight ½e). Correct width (½) 6mm (to within 2mm)(f). Even in width (1)(g). Seam well pressed flat (½) on R.S ½) and W.S(½) | ½ 1½ 1½  11½  |  |  |
|  | **Sub Total** | 7 ½ marks |  |  |
| 4 | **OPEN SEAM – SIDE SEAM**If not open seam award ‘0’(a). Seam jointed with straight stitchery (1 ½ )(b). Well neatened (½) raw edges(c). Evenness (1½) of seam allowances i.e. 1cm to within 2mm(e). Seam well pressed open (1) and flat on R.S (1 ½ ) and W.S(1) | 1½½1 ½½3 ½  |  |  |
|  | **Sub total** | 7 ½  |  |  |
| 5 | **PREPARATION AND ATTACHMENT OF THE COLLAR**(a). Collar correctly interfaced (½)(b). Collar pieces trimmed (½)(c). Collar well knife edged (½)(d). Correct size (½) and shape (½) of collar 1 1(superimposed)(e). Collar top stitched (½) neatly and correctly(f). Facing well edge stitched (½)(g). Collar sandwiched between garment and facing at the front (½)(h). Smooth stitchery (½) along neckline seam on seam line 1/2 (i) Neckline seam trimmed (1 ½ layer and snipped (½)(j). Correct positioning of collar (½) (2)(k). Correctly pressed flat (½) and facing (½) turned to 1 W.S (½) of garment. Front finished using facing back ½ self-neatened (1)(l) Facing flat and catch stitched (½) along shoulder ½ seam(½) |  |  |  |
|  | **Sub total 10 ½ marks** |  |  |  |
| 6 | (a). Pocket hem turned to W.S (½) and raw edges folded under (1½) (b). Seam trimmed (1) correct width of the hem(1)(c).Pocket hem machine top stitched (1 ½ ) straight (½)(d). Evenness of the pocket hem (½) (e). Correctly attached into position (½) with straight stitchery (½) close to the fold (½) (f). Top corners well reinforce (½)(g). Pocket edges well tucked under (½)(h). Correct size (½) and shape (½) of pocket (superimposed) | 222½1½½½1 |  |  |
|  | **Sub total** | 10 marks  |  |  |
| 7 | **HEM MANAGEMENT**(a). Edge stitching done (½)(b). Evenness of the hem(½)(c). Correctly done with slip hemming (½) stiches(d). Quality of slip hemming stiches worked (1)(e). Hem pressed flat (1)(f). Facing correctly managed at the hem line (machined trimmed corner snipped and pushed out knife edge)(1) | ½½½111 |  |  |
|  | **Sub total** | 4 ½  |  |  |
| 8 | **BUTTON HOLE**(a). Button hole cut (1) on straight grain (1)(b). Well-made buttonhole even stitched (1)(c). Buttonhole stiches used (1)(d). quality of buttonhole stich (1) tension and density(e). Edges of buttonhole well stitched (1)(f). Correct size 2cm (½) and position (½) of buttonhole | 211111 |  |  |
|  | **Sub total** | 07  |  |  |
| 9 | **PREPARATION AND ATTACHMENT OF THE SLEEVE**(i). Insertion gap 1.5cm a centimeter away from sleeve seam (2)(ii). Gathers stiches worked using machine from notch to notch(3)(iii). Setting-in-sleeve into armhole. With smooth stitchery.(2)(iv). Notches matching (2)(v). Underarm seam matching side seam (1)(vi). Well inserted elastic band (1) and well finished (1) |  232212 |  |  |
|  | **Sub total** | 12 marks |  |  |
| 10 | **FISHBONE STITCH**(a).Well cut size tear (1)(b). Fishbone stitch work (2)(c). Loops formed at ends of stitches (2)(d). Neat stitchery (1) | 1221 |  |  |
|  |  | 06 |  |  |
|  | **WORK MANSHIP** | 04 ½ marks |  |  |
|  | **Grand Total** | **90** |  |  |
|  | ÷2 | **45** |  |  |