DECEMBER EXAM HOME SCIENCE PAPER 2 MAKING SCHEME.

CANDIDATE NAME\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_INDEX \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

|  |  |  |  |
| --- | --- | --- | --- |
|  | ACTIVITY | SCORE | STUDENT SCORE |
| 1. | PRESENTATION |  |  |
| a).  b).    c.  d. | Work well pressed (1) and folded ( ½ )  Label ( ½ ) firmly stitched (1) without concealing details ( ½ ) and on single fabric ( ½ )  Pins/needle ( ½ ) and unnecessary tacking threads ( ½ ) removed  Made up for the LEFT side | 1 ½  2 ½  1 ½  1 |  |
|  |  | 6 ½ |  |
| 2.  a).  b).  c).    d).  e)  f).  g).  h).  i). | CUTTING OUT  All eight pieces ( ½ x8) cut out  Smooth cutting of CF of bodice   1. And on straight grain to within 3mm (1)   Smooth cutting of the CB of bodice (1) and cut on straight grain to within 3mm(1)  Smooth cutting of CF of Skirt  Smooth cutting of CB of skirt  Smooth cutting of the dress lower edge front (1) and back (1)  Smooth cutting of the sleeve edge  Crossway strip cut on true bias  Dress skirt cut on true bias front ( ½ ) and back ( ½ ) | 4  2  2  1  1  2  1  1  1 |  |
|  |  | 15 |  |
| 3. | DART |  |  |
| a)  b).  c).  d).  e). | Straight stitchery ( ½ ) of dart and tapering to nothing ( ½)  Stitching fastened at the point  Correct length of the dart 7.5cm to within 2mm (7.3cm-7.7cm)  Correct width of dart 1.5cm to within 2mm (1.3cm – 1.7cm)  Pressed towards CB  Flatness of dart on w.s ( ½ )and R.S ( ½ ) | 1 ½  ½  1  1  1  1 |  |
|  |  | 6 |  |
| 4. | SHOULDER SEAM –DOUBLE STITCHED  (if not double stitched award zero) |  |  |
| a).  b).  c).  d).  e).  f). | First row of stitchery made with straight stitches.  Raw edges well tacked under  Second line of stitchery made with straight stitches  Evenness of seam (1) and correct size 0.6cm to within 2mm (1) (0.4cm – 0.8cm)  Flatness of seam on R.S (1) and on W.S (1)  Fell facing back of dress | 1  1  1  2  2  1 |  |
|  |  | 8 |  |
| 5.  a).  b).  c).  d).  e).  a).  b).  c).  d).  e). | SIDE SEAMS – OPEN SEAM  If not open seam award zero (0)  BODICE  Joined with straight stitchery  Raw edges well neatened (1x2)  Evenness of seam allowance  Correct size of seam allowance 1cm to within 2mm (0.8-1.2cm)  Seam pressed open and flat at the arm hole (1) and waist (1)  SKIRT  Joined with straight stitchery  Raw edges well neatened (1x2)  Evenness of seam allowance  Correct size of seam allowances  1cm to within 2mm (0.8-1.2cm)  Seam pressed open and flat at waist | 1  2  1  1  2  1  2  1  1  1 |  |
|  |  | 13 |  |
| 6.  a).  b).  c).  d).  e). | WAIST SEAM –PLAIN SEAM  Joined with straight stitchery  Seam evenly trimmed (1) and correct size (1) 1cm to within 2mm (0.8cm -1.2cm)  Loop stitches (1) made on half back (1)  Quality of loop stitches ie evenly distributed ( ½ ) correct tension ( ½ ) even length thread ( ½ )  Side seam meeting to within 2mm  CB of bodice and CB of skirt flash ( ½ )  CF of bodies and CF of skirt flash ( ½ ) | 2  2  2  2  1  ½  ½ |  |
|  |  | 10 |  |
| 7. | COLLAR |  |  |
| a).  b).  c).  d).  e).  f).  g).  h).  i).  j).  k). | Smooth stitchery of outer edge of color(mark by impression)  Collar seam trimmed (1) and snipped (1)  Well knife edged collar  Collar attached by sandwiching in the dress and crossway strip  Quality of attaching stitchery (mark by impression on R.S)  Attaching seam trimmed (1) and snipped (1)  Crossway strip held down with straight stitchery (1)and well tucked under (1)  Evenness of the crossway strip  Correct positioning of collar ie CF of collar flash with C.F of Bodice (1) and CB of collar 1.5cm from cutting edge (1)  Correct size (1) to within 5mm and correct shape (1)  (superimpose pattern)  Collar lying flat on dress front ( ½) and dress back ( ½ )  C.F of crossway strip and C.F of bodice flash ( ½ ) and CB of crossway strip and CB of bodice flash ½ | 1  2  1  1  1  2  2  1  1  1  2  1  1 |  |
|  |  | 17 |  |
| 8. | **UNDERARM SEAM – OPEN SEAM** |  |  |
| a). | Joined with straight stitchery  Raw edges well neatened (1x2)  Evenness of seam allowance  Correct size of seam allowance 1cm to within 2mm (0.8cm – 1.2cm)  Seam pressed open and flat at the armhole | 1  2  1  1  1 |  |
|  |  | 6 |  |
|  | SLEEVE |  |  |
| a) | Good hang  Gathers (1) evenly distributed (1) at the crown ( ½ )  Armhole made with straight stitchery  Armhole seam neither trimmed ( ½ ) nor neatened ( ½ )  Correct position ie front notches ( ½ ) and back notches ( ½ ) matching  Underarm seam and side seam matching to within 2mm | 1  2 ½  2  1  1  1 |  |
|  |  | 8 ½ |  |
|  | TOTAL | 45 |  |