ASUMBI GIRLS HIGH SCHOOL

POST -MOCK 1

AUGUST/SEPTEMBER

2022

**HOME SCIENCE PP2 MS**

MARKING SCHEME

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | PROCESS | MAX SCORE | SCORE | REMARKS |
| 1abcd | **PRESENTATION**Work well pressed (1) and folded (**1/2**)Label (1) firmly fixed (1) on single (**1/2**) fabric without concealing details (**1/2**) Pins (**1/2**) needles (**1/2**) tacking, unnecessary threads (**1/2**) removedMade for the right half (1) | 1**1/2**2**1/2**1**1/2**1 |  |  |
|  | Sub – Total | 6**1/2** |  |  |
| 2abcdef | **CUTTING OUT**All the 6 pieces cut out (3)Smooth cutting of the dress CF (2) on grain (2)Smooth cutting of dress CB (2) on grain (2)Smooth cutting of the front facing (**1/2**) on grain (**1/2**)Smooth cutting of back neck facing CB (**1/2**) on grain (**1/2**)Smooth cutting of the dress lower edge 1 × 2 (2) | 344112 |  |  |
|  | Sub – Total | 15 |  |  |
| 3abcd | **MAKING OF THE DOUBLE POINTED DART**Dart made with smooth stitchery (1) tapering to points on the fold **1/2** × 2 (1) secured at the end (1)Dart slashed in the middle (**1/2**) and neatened (1) Correct length of the dart 10cm to within 5mm (9.5cm – 10.5cm) (1)Correct width of the dart 1cm to within 2mm (0.8cm – 1.2cm) (1) | 31**1/2**11 |  |  |
|  | Sub – Total | 6**1/2** |  |  |
| 4abcde | **THE MAKING OF THE OPEN SEAM AT THE SHOULDER** **(**Award zero if not open seam)Seam joined with straight stitchery (1)Seam neatened (2)Evenness of the seam (1)Correct size of the seam 1cm to within 2mm (0.8cm – 1.2cm) (1)Seam open and flat at the shoulder RS (1) WS (1) and at the armhole RS (1) WS (1) | 12114 |  |  |
|  | Sub total | 9 |  |  |
| 5abcdefg | **MAKING OF FRENCH SEAM AT THE SIDE OF THE DRESS**(Award zero if not French seam)First row made with straight stitchery (1**1/2**)Second row made with straight stitchery (1**1/2**)Seam well knife edged (2)Correct size of seam 6mm to within 2mm (4mm- 8mm) (1)Seam allowance trimmed (1) no threads showing on the RS (1)Evenness of the seam (1)Seam pressed to the back at armhole | 1**1/2**1**1/2**21211 |  |  |
|  | Sub – Total | 10 |  |  |
| 6IabcdefIIabcdefghijkl | **PREPARATION OF THE SLEEVE**First row joined with straight stitchery (1)Second row joined with straight stitchery (1)Row edges trimmed (**1/2**) and concealed (**1/2**)Seam knife edged (1)Correct size of seam 6mm to within 2mm (4mm- 8mm) (1)Seam pressed towards the back at the band (**1/2**) and armhole (**1/2**)Band seam joined with straight stitchery (1) seam trimmed (**1/2**) and pressed openGathers (1) well distributed between the marks (dots) (1)Armband flat (**1/2**)Underarm seam and armband seam flash (**1/2**)Evenness of the band (1)Correct width of the armband 4cm to within 2mm (3.8cm – 4.2cm) (1)Hemming(Award zero from f if not hemming stitches)Hemming stitches uniform in size (1)Well distributed (1)Correct tension (1)Worked on single thread (1)Stitches not visible on RS (1)Stitches secured at the beginning (1) and at the end(1) | 11111122**1/2**11111112 |  |  |
|  | Sub – Total | 20 |  |  |
| 7abcd | **ATTACHING THE SLEEVE DO NOT NEATEN THE SLEEVE**Good hang of the sleeve (1)Sleeve attached with smooth stitchery (2)Notches (2) matched (1)Gathers (1) well distributed (1) at the crown (1) | 1233 |  |  |
|  | Sub – Total | 9 |  |  |
| 8ab | **JOINING OF THE FRONT AND BACK NECK FACINGS**Facing joined with straight stitchery (1)Seam trimmed (1) and pressed open (1) | 12 |  |  |
|  | Sub – Total | 3 |  |  |
| 9abcdef | **ATTACHING OF THE FACING TO NECKLINE AND NEATENING THE FREE EDGES**Facings joined to neckline with straight stitchery (2)Seam trimmed (1) and notched (1)Facings edge stitched at free edge (2)Facings held on the dress with catch stitches at CF (**1/2**) CB (**1/2**) and shoulder (**1/2**)Facing flash with garment at CF **1/2** × 2 (1) shoulder **1/2** × 2 (1) and CB **1/2** × 2 (1)Facings flat on the garment (1) | 2221**1/2**31 |  |  |
|  | Sub – Total | 11**1/2** |  |  |
|  | TOTAL | 90 |  |  |
|  | TO GET FINAL SCORE DIVIDE BY 2 (90 ÷ 2) |  |  |  |