**FORM FOUR**

**END OF SECOND TERM EXAMINATIONS**

**CLOTHING CONSTRUCTION**

**HOMESCIENCE PAPER 2**

**MARKING SCHEME**

**AUGUST/SEPTEMBER 2022**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **ACTIVITY** | **SCORE** | **MAXIMUM** **SCORE** | **REMARKS** |
| 1 | **PRESENTATION** |  |  |  |
| a)b)c) d) | Work well pressed (1) and folded (1/2)Label (1/2) firmly (1/2)fixed without concealing details (1/2) and on a single fabric (1/2)Pins/needles(1/2) and unnecessary tacking threads (1/2) and loose threads (1/2) removed Made up for the LEFT HALF (1) | 11/2211/21 |  |  |
|  | **Sub-Total**  | **61/2** |  |  |
| **2** | **CUTTING OUT** |   |  |  |
| a)bcdefgh,i | All eight pieces cut out ( 1/2 x 8) Smooth cutting of the C.F of bodice (1) and cut on straight grain to within 3mm(1)Smooth cutting of the C.B of bodice (1) and cut on straight grain to within 3mm(1)Smooth cutting of C.F of skirtSmooth cutting of C.B of skirtSmooth cutting of dress lower edge front(1) and back(1)Smooth cutting of sleeve edge (1)Cross way strip cut on true biasDress cut on true bias front(1/2) back(1/2 ) | 422112111 |  |  |
|  | **Sub-Total** | 15 |  |  |
| 3 | **DART** |  |  |  |
| a)b) c)d)e) f) | Straight stichery (1) of dart and tapering to nothing(1/2)Stitchery fastened at the point(1/2) Correct length of the dart 7.5 cm to within 2mm(7.3cm to 7.7cm)(1)Correct width of dart 1.5cm to within 2mm(1.3cm-1.7cm) (1) Pressed towards C.F(1)Flattness of dart on W.S (1/2) and R.S (1/2) | 11/2½1111 |  |  |
|  | **Sub-Total** | **6** |  |  |
| 4.a)b)c)d)e)f) | **SHOULDER SEAM -DOUBLE STITCHED SEAM- If not double stitched award zero** First row of stitchery made with straight stitches(1)Raw edges well tucked under(1)Second line of stitchery made with straight stitches (1)Evennes of seam (1) and correct size 0.6cm to within 2mm(1)(0.4-0.8cm)Flatnnes of seam on the R.S(1) and on W.S(1)Fell facing back of dress(1) | 111221 |  |  |
|   | **Sub-Total** | **8** |  |  |
| 5. | **SIDE SEAM -OPEN SEAM If not open seam award zero.** |  |  |  |
| a)b)c)d)e)f)g)h)i)j) | **BODICE**Joined with straight stitchery(1)Raw edges well neatened (1x2)Evenness of seam allowance(1)Correct size of seam allowance 1cm to within 2mm(0.8-1.2cm) (1)Seam pressed open and flat at armhole(1) and waist(1)**SKIRT**Joined with straight stitchery(1)Raw edges well neatened(1x2)Evenness of seam allowance(1)Correct size of seam allowance (1cm) to within 2mm(0.8-1.2cm)(1)Seam pressed open and flat at the waist(1) | 1211212111 |  |  |
|  | **Sub –Total** | **13** |  |  |
| 6.a)b)c)d)e)f) | **WAIST SEAM- PLAIN SEAM****If not plain award zero**Joined with straight stitchery (2)Neatened section evenly trimmed(1) and correct size(1) (1cm to within2mm(0.8-1.2cm)(2)Loop stitches(1)made on half back (1)Quality of loop stitches; Evenly distributed(1/2)correct tension(1/2) even length(1/2)and worked using single thread(1/2)Side seeams meeting to within 2mm on the R.S(1) C.B of bodice and C.B of skirt flash (1/2)to within 2mmC.F of bodice and C.F of skirt flash (1/2)to within 2mm | 222211 |  |  |
|  | **Sub –Total** | **10** |  |  |
| 7a)b)c)d)e)f)g)h)i) j)k)i) | **COLLAR**Smooth stitchery of outer edge of collar(mark by impression(1)Collar seam trimmed (1)and snipped(1)Well knife edged collar(1)Collar attached by sandwiching in the dress and crossway strip(1)Quality of attaching stitchery(mark by impression on R.S(1)Attaching seam trimmed(1) and snipped(1)Crossway strip held down with straight stitchery(1) and well tucked under(1)Evenness of crossway strip(1)Correct positioning of collar i.e C.F of collar flash with C.F of bodice(1) extension and C.B(1/2)of collar 1.5cm from cutting edge(1/2)Correct size of collar (1) to within 5mm and correct shape(1)(superimpose patternCollar lying flat on dress front(1/2)and dress back(1/2)C.F of crossway strip and C.F of bodice flash(1/2)and C.B of crossway strip and C.B flash(1/2)to within 2mm | 121112212211 |  |  |
|  | **Sub –Total** | **17** |  |  |
| 8. | **UNDERARM SEAM- OPEN SEAM** |  |  |  |
| a)b)c)d)e) | Joined with straight stitchery (1)Raw edges well neatened(1x2)Evenness of seam allowance(1)Correct size of seam allowance 1cm to within 2mm(0.8-1.2mm)(1)Seam pressed open (1/2)and flat(1/2)at the armhole on the W.S | 12111 |  |  |
|  | **Sub-Total** | **6** |  |  |
| 9a)b)c)d)e)f) | **SLEEVE**Good hang (1)Gathers(1) evenly distributed(1) at the crown (1/2)Armhole made with straight stitchery (2)Armhole seam neither trimmed(1/2)nor neatened(1/2)Correct position i.e front notches(1/2)and back notches(1/2)Underarm seam and side seam matching to within 2mm(1) | 121/22111 |  |  |
|  | **Sub – Total** | 81/2 |  |  |
|  | **GRAND TOTAL** | 90/2 |  |  |
|  |  | 45 |  |  |
|  |  |  |  |  |