**441/2**

**HOMESCIENCE CLOTHING CONSTRUCTION**

**PAPER 2**

**(PRACTICAL)**

**JUNE - 2022**

**TIME 2 ½ HRS**

**NAME.................................................................. ADM NO............................. CLASS.................**

**BUNAFAM CLUSTER EXAMS – 2022**

**MARKING SCHEME**

**HOME SCIENCE PAPER 441/2 PRACTICAL MARKING SCHEME**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **AREA OF ASSESMENT** | **MAXIMUM SCORE** | **ACTUAL SCORE** | **REMARKS** |
| 1 | **PRESENTATION**   1. Work well pressed (1) and folded (½ ) 2. Label ( ½ ) firmly Fixed (1) without concealing details ( ½ ) and on single fabric ( ½ ) 3. Pins /needles( ½ ) tacking thread ( ½ ) and unnecessary thread removed 4. Made up for the Left half (1) | 1 ½  2 ½  1 ½  1 |  |  |
| **SUB- TOTAL** | **6 ½** |  |  |
| 2 | **CUTTING OUT**   1. All 6 pieces cut out 6x½ 2. Smooth cutting of skirt back C.B 1x2 3. Straight grain of skirt C.B to within 3mm 4. Smooth cutting of front skirt yoke CF 1x2 5. Straight grain of skirt C.F to within 3mm 6. Smooth cutting of frills C.F 1x2 7. Straight grain of frills to within 3mm 8. Smooth cutting of Front waist Band 9. Smooth cutting of Back waist Band | 3  2  1  2  1  2  1  1  1 |  |  |
| **SUB – TOTAL** | **14** |  |  |
| 3 | **MAKING UP**  The making of the dart at the back skirt   1. Dart required length 4.6cm and width (7mm) 2. Tapering to nothing at the end and no pockets 3. Dart well reinforced 4. Stitched from the wide side 5. Flat at the waist Band ( ½ ) and facing towards (C.B) ( ½ ) 6. Dart made on W.S( ½ ) | 2  1  1  1  ½  ( ½ ) |  |  |
| **SUB-TOTAL** | **14**½ |  |  |
| 4 | **JOINING OF THE YOKE FRONT TO HEM LOWER SKIRT**  **FRONT:** givezero if not over laid seam  Skirt front yoke joined to the skirt with straight stitchery close to the fold.   * Front seam allowance even * Yoke and skirt flash at C.F to within 3mm   **Loop stitches**   * Neatening of half of the front seam with loop stitches. * Straight stitches * Correct tension * Evenness of stitches * Correct size of neatening 1 depth of loop 3mm to 0.5mm * Fastening ( reinforcing with Back stitches on both ends * Quality of work man ship | 2  1  1  1  1  1  1  1  1 |  |  |
| **SUB-TOTAL** | **12** |  |  |
| 5 | Attaching of the frill to the lower skirt front using a plain seam. **(Leave the gathering stitches and do not trim the seam allowance.)**   * If not plain seam give zero * Frills attached with straight stitchery   Gathers evenly distributed (2) and gathering stitches not removed (1)   * Seam allowance not trimmed * Frills of skirt flash at (C.F)   **Plain seam**   * Straight stitchery * Evenness of width * Neatening of Raw edges together * Correct tension | 2  3  1  1  1  1  1  1 |  |  |
| **SUB -TOTAL** | **11** |  |  |
| 6 | **Making of the skirt side seam from the yoke to the hemline using an open seam.**   * If not open seam give zero * Seam joined with straight stitchery ( 1 ½ ) and well secured at the waist Band (1/2 ) * Seam appropriately neatened (1x2) * Evenness of seam allowance ½ x2 * Correct width 1cm to within 2mm on either side (0.8cm – 1.2 cm ( ½ x 2) * Seam pressed open and flat at waist Band. | 2  2  1  1  1  1 |  |  |
| **SUB -TOTAL** | **7** |  |  |
| 8 | **Attaching of the front and back waistbands and holding them in place using tacking – stitches**   * Front waist Band joined with back waist band. * Interfacing the front waist band and back Waist Band. * Straight stitchery of the joining seam. * Joining the waistband to the skirt front and skirt back using straight stitchery * Seam allowance evenly trimmed (2) and Raw edges of waist band neatly tucked under (1) using tacking stitches (1) * Eveness of width of waist band both on the W.S and R. S * Flatness (1) of waist band and well top stitched (1) and knife edged (1)   TUCKING STITCHES   * Correct stitches made * Good stitchery (1) straight stiching * Correct tension * Correct length and width 1cm to within 2mm | 1  2  1  3  1  2  3  1  2  1  2 |  |  |
|  | **SUB TOTAL** | **21** |  |  |
|  |  |  |  |  |
| 9 | **MAKING OF THE HAND WORKED BUTTON HOLE if not stitch award zero**   1. Correct position (1) and size (1) of button hole 2. Button hole cut straight (1) and worked with single thread (1) 3. Button hole worked with even (1) and well distributed (1) button hole stitches   Either   1. Round and worked with well distributed (1) button hole stitches (1) **or** 2. Square and completed with a bar (1) worked with even button hole stitches (1) 3. Raw edges concealed by the button hole on the right side 4. Flatness of button hole | 2  2  2  2  2  2  2 |  |  |
|  | **SUB TOTAL** | **12** |  |  |
|  | **GRAND TOTAL MARKS** | **90** |  |  |
|  | **FINAL MARK = ACTUAL MARK**  2 | **45** |  |  |