**PANGANI POST MOCK EXAMINATION**

**2022**

**MARKING SCHEME**

MARKING SCHEME

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | PROCESS | MAX  SCORE | SCORE | REMARKS |
| 1  a  b  c  d | **PRESENTATION**  Work well pressed (1) and folded (1/2)  Label (1) firmly fixed (1/2) on single fabric (1/2) without concealing details (1/2)  Pins (1/2) needles (1/2) tacking stitches and unnecessary threads (1/2) removed  Made for the right half (1) | 11/2  21/2  11/2  1 |  |  |
|  | Sub – Total | 61/2 |  |  |
| 2  a  b  c  d  e  f | **CUTTING OUT**  All the six pieces cut (3)  Smooth cutting of the bodice C front (1) on grain (1)  Smooth cutting of the bodice CB (1) on grain (1)  Smooth cutting of yoke CF (1/2) on grain (1/2)  Smooth cutting of collar CF (1) on bias (1)  Smooth cutting of bodice lower edge front (1) back (1) | 3  2  2  1  2  2 |  |  |
|  | Sub – Total | 12 |  |  |
| 3  a  b  c | **ATTACHING OF THE YOKE TO THE BODICE BACK WITH AN OVERLAID SEAM DO NOT NEATEN THE SEAM**  Seam joined with straight stitchery (1) close to the fold (1) raw edges well tucked under (1)  Notches (1) matched (2)  Bodice and yoke flash at CF (1/2) | 3  3  ½ |  |  |
|  | Sub – Total | 61/2 |  |  |
| 4  a  b | **THE WORKING OF THE WAIST DART**  Dart joined with straight stitchery (1) tapering to a point on the fold (1/2) and secured at the end (1/2)  Correct length of the dart 8.5cm to within 2mm (8.3cm – 8.7cm) (1/2) and correct width of the dart 1cm to within 2mm (0.8cm – 1.2cm) (1/2) | 2  1 |  |  |
|  | Sub – Total | 3 |  |  |
| 5  a | **THE NEATENING OF THE RAW EDGES OF THE FRONT FACING**  Facing edge stitched (1) with smooth stitchery (1) close to the fold (1) | 3 |  |  |
|  | Sub – Total | 3 |  |  |
| 6  a  b  c  d  e  f  g | **THE JOINING OF THE SHOULDER SEAM USING MACHINE FELL SEAM**  (Award zero if not machine fell seam)  First row joined with straight stitchery (1)  Second row joined with straight stitchery (1) close to the fold (1/2) with raw edges well tucked under (1/2)  Correct size of the seam 6mm to within 2mm (4mm -8mm) (1)  Evenness of the seam (1)  Seam made on the RS (1)  Seam fell turned to the back side (1)  Seam flat on RS (1/2) and WS (1/2) | 1  2  1  1  1  1  1 |  |  |
|  | Sub – Total | 8 |  |  |
| 7  a  b  c  d  e  f  g  h | **THE ATTACHING OF THE COLLAR INCLUDING THE PREPARATION OF THE COLLAR EXTENSION**  Collar joined with straight stitchery (1)  Seam trimmed (1) and pointed at the corners (1)  Collar knife edged (1)  The attaching seam is smooth (1) trimmed (1) and notched at the neckline (1)  Collar finished with even hemming stitches (1)  Correct tension of stitches (1/2) neatly secured at the end (1/2)  Collar even in size (1) and flat (1)  Collar flash with yoke and CB 1/2 × 2 (1) | 1  2  1  3  1  1  2  1 |  |  |
|  | Sub – Total | 12 |  |  |
| 8  a  b  c  d  e | **THE JOINING OF THE SIDE SEAM USING AN OPEN SEAM**  (Award zero if not open seam)  Seam joined with straight stitchery (1)  Seam neatened (2)  Correct size of the seam 1cm to within 2mm (0.8cm – 1.2cm) (1)  Evenness of the seam (1)  Seam open and flat at armhole on RS (1) and WS (1) | 1  2  1  1  2 |  |  |
|  | Sub – Total | 7 |  |  |
| 9  a  b  c  a  b  c  d  e  a  b  c  d  e  f  g  h | **PREPARATION OF THE SLEEVEUSING OPEN SEAM AT UNDERARM**  (Award zero if not open seam)  To include:  Underarm seam joined with straight stitchery (1)  Seam neatened (1)  Seam pressed open and flat at the underarm on RS (1/2) and WS (1/2) and at the facing on the RS (1/2) and WS (1/2)  i) **The preparation and attaching of the facing to the sleeve right side**  Facing ends with straight stitchery (1/2) seam trimmed (1/2) and pressed open (1/2)  Facing attached to the sleeve with straight stitchery (1)  Seam trimmed (1)  Facing top stitched on the sleeve RS (1) close to the fold(1) with raw edges well tucked under (1)  Facing seam flash with underarm seam 1/2 × 2 (1)  ii) **Attaching of the sleeve to the armhole and neatening half of the armhole seam**  Good hang of the sleeve (1)  Sleeve joined with smooth stitchery (2)  Notches (1) at the untrimmed section and matched (1)  Neatened section trimmed (1)  Neatened with uniform stitches (1/2) evenly (1/2) distributed  Stitches secured at the ends 1/2 × 2 (1)  Gathers (1) well distributed (1) at the crown (1)  Underarm seam and side seam flash (1/2) | 1  1  2  11/2  1  1  3  1  1  2  2  1  1  1  3  ½ |  |  |
|  | Sub – Total | 23 |  |  |
| 10  a  b  c  d  e  f | **THE WORKING OF THE BUTTONHOLE**  Buttonhole cut on grain (1) correct size of the buttonhole 1.4cm to within 2mm (1.2 cm – 1.6cm) (1)  (Award zero from b if not button hole stitches )  Stitches made on single thread (1) equal in length (1) and evenly distributed (1)  Correct tension of the stitches (1)  Rounded end correctly made (1)  Stitches neatly made on the WS (1)  Threads secured at the end (1) | 2  3  1  1  1  1 |  |  |
|  | Sub – Total | 9 |  |  |
|  | Total | 90 |  |  |
|  | **FIND THE FINAL MARK BY DIVIDING BY 2 (90 ÷ 2)** |  |  |  |