**FORM 4 HOMESCIENCE EXAM END TERM 2 2024**

**441/2 PAPER 2 MARKING SCHEME**

|  |  |  |  |
| --- | --- | --- | --- |
|  | **ACTIVITY** | **SCORE** | **Maximum score** |
| 1 | **PRESENTATION** |  |  |
| a) b) c) d)  | Work well pressed (1) and folded ( ½ )Label ( ½ ) firmly stitched (1) without concealing details ( ½ ) and on a single fabric ( ½ )Pins/needles ( ½ ) and unnecessary tacking threads ( ½ ) and loose threads ( ½ ) removedMade up for the Right half 1 | 1 ½ 2 ½ 1 ½ 1 |  |
|  |  | 6 ½  |  |
| 2 | **CUTTING OUT** |  |  |
| a) b)c)d)e)f) | All eight pieces ( ½ x8) cut outSmooth cutting of the C.B on dress (2) and cut on straight grain to within 2 mm (1)Smooth cutting of the dress lower edge front (1) and back (1) Smooth cutting of the sleeve edge (1)Sleeve strip cut on grain (1)Smooth cutting of collar C.B. ( ½ x 2 ) and out on grain( ½ x2) | 432112 |  |
|  |  | 13 |  |
| 3 | **NECK DART** |  |  |
| a)b)c)d)e)f) | Straight stitchery (1) of dart and tapering to nothing ( ½ )Stitchery fastened at the pointCorrect length of the dart 8 cm Correct width of dart 0.7cm Pressed towards C.BFlatness of dart on W.S ( ½ ) and R.S ( ½ ) | 1½ ½1111 |  |
|  |  | 6 |  |
| 4 | POCKET |  |  |
| a)b)c)d)e)f)g) | Preparation of pocket mouth 1 even hem (½) and straight stitchery ½ Pocket turning well tucked ( ½ x3 )under evenly trimmed( ½ x3) and snipped ½ at the basePocket fixed with straight stitches (1 x 3) and close to the edge ( ½ x 3)Pocket reinforced at the mouth corners (½ x2 )Correct positioning of the pocket1Correct size 1and correct shape1Flatness of pocket on RS ½ and WS ½  | 23 ½ 4 ½ 1121 |  |
|  |  | 15 |  |
| 5 | **SHOULDER SEAM – OPEN SEAM (if not OPEN SEAM award zero (0)** |  |  |
| a)b)c)d)  | Joined with straight stitcheryRaw edges well neatened (1x2)Evenness of seam allowanceCorrect size of seam allowance 1cm (1 X 2)Seam pressed ½ open ½ and flat at the neck edge ½ and shoulder(1/2 )  | 12122 |  8 |
| **6** | **SIDE SEAMS – OPEN SEAM****(if not open seam award zero (0)** |  |  |
| a)b) c)d)e) | joined with straight stitcheryRaw edges well neatened (1x2)Evenness of seam allowanceCorrect size of seam allowance 1cm Seam pressed open and flat at the arm hole (1) and waist (1) | 12112 |  |
|  |  | 7 |  |
| 7 | **NECK FACING** |  |  |
| a)b)c) | Back and front facing joined with straight stitches (½)Seam trimmed ( ½ )pressed open (½ )and unneatened (½ )Free edge of facing well neatened( 2 )and held down ½ at shoulder seamline( ½ ) | ½ 1 ½ 3 |  |
|  |  | 6 |  |
| 8.  | **COLLAR** |  |  |
| a)b)c)d)e)f)g)h)i)j) | Smooth stitchery of outer edge of collar (mark by impression)Collar seam trimmed (1) and snipped (1)with sharp point ½ Well knife-edged collarCollar attached by sandwiching in the dress and facingQuality of attaching stitchery (mark by impression on R.S)Attaching seam trimmed (1) and snipped (1)Evenness of the facingCorrect positioning of collar i.e. C.F on collar flash with C.F. of bodice (1/2 ) and C.B of collar flash with CB of dress (1/2)Correct size (1) to and correct shape (1) (superimpose pattern)CB of facing and CB of dress flash | 12 ½ 1112112½  |  |
|  |  | 13 |  |
| 9 | **CONTINOUS WRAP OPENING ( if not continuous wrap award zero** |  |  |
|  a)b)c)d)e)f)  | Quality of the attaching stitches (½ x 2)Quality of the neatening of the strip on the WS raw edges well tucked under (½ x 2)Well fixed with hemming stitches( ½ x 2)Folding of the back strip to WS ½ and backstitching at the base ½ Evenness of the strip (1)Correct size of opening 8cm (½ x 2)  | 111111 |  |
|  |  | 6 |  |
| 10. | **UNDERARM SEAM – FRENCH SEAM If not french seam award zero** |  |  |
| a)b)c)d)e) f)g)h)i) | Seam made before sleeve is attached Straight stitchery of seamSeam well trimmed no threads on RSSeam well knife edgedEvenness of the seamCorrect size 6mm to within 2mm (4- 8mm)Seam pressed towards the back of the armholeFlatness of seam at armhole RS and WSSide seam and underarm seam meeting | ½ ½ 1111½ 1½  |  |
|  |  | 7 |  |
| 11 | **SLEEVE** |  |  |
| a)b)c)d)e)f) | Good hang (2)Gathers well distributed (1) at the crown (1)Armhole seam made with smooth stitchery (1)Correct positioning of the sleeve i.e. back to back (1) front to front (1)Notches match at the armhole seam (1x2)Underarm seam meeting with side seam  | 221221 |  |
|  |  | 10 |  |
|  | **GRAND TOTAL** | 90 /2 = 45 |  |