**BONDO SUB-COUNTY JOINT EXAMINATION 2021**

**HOME SCIENCE PAPER 2**

**MARKING SCHEME**

**Name:……………………………………….. Index No.:………………………..**

**School:………………………………………. Date:………………………….**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **AREA OF ASSESSMENT** | **MAX SCORE** | **SCORE** | **REMARKS** |
| 1 | **PRESENTATION**1. Work well pressed (½)
2. Well folded (½)
3. Label firmly fixed (½) without concealing details on a single layer of fabric (½)
4. Pins and needles ( ½) and unnecessary tacking threads ( ½) removed
5. Made up the right half
 | 1111 |  |  |
|  |  | **04** |  |  |
| 2 | **CUTTING OUT**1. All eight pieces cut out (½ x 8)
2. Smooth cutting (1) of the dress front and to the grain (1)
3. Smooth cutting (1) of the dress back and to the grain (1)
4. Sleeve smoothly cut (1) and to the grain (1)
5. Front yoke smoothly cut (1) and to the grain (1)
6. Collar smoothly cut (1) and to the grain (1)
7. Front neck facing smoothly cut (½) and on grain (½)
8. Back neck facing smoothly cut (½) and on grain (½)
9. Frill smoothly cut (1) and on fold (1)
 | 422222112 |  |  |
|  |  | **18** |  |  |
| 3 | **DART**1. Dart worked using straight stitching
2. Machined tapering to nothing
3. Ends well reinforced
4. Correct length and width
5. Pressed towards CB
6. Flat on R.S & W.S
 | 111111 |  |  |
|  |  | **06** |  |  |
| 4 | **OVERLAID SEAM ON YOKE**(***If not overlaid award zero***)1. Yoke overlaid on the dress
2. Machine close to the fold ( ½) on the R.S (½)
3. Straight stitching (½)
4. Trimmed to 1cm (½)
5. Overcastting stitches used (1)
6. Evenly spaced (1) and neat (1)
 | 11½ ½ 12 |  |  |
|  |  | **06** |  |  |
| 5 | **MACHINE FELL SEAM AT THE SHOULDER** (***If not machine fell award zero***)1. First (1) and second (1) rows straightly stitched
2. Correct width of seam 0.6cm
3. Evenness of the fold
4. Fell lying towards the back (1) well tacked under (1)
5. Flat on R.S and W.S
 | 21121 |  |  |
|  |  | **7** |  |  |
| 6 | **FRENCH SEAM AT THE SIDE SEAM AND UNDERARM SEAM X2** (*If not French seam award zero*)1. Correct width (1) and even (1)
2. Raw edges enclosed (1)
3. Straight stitchery (½) correct tension (½)
4. Good knife edge (1)
5. Pressed flat (½) towards the back (½)
 | 21111 |  |  |
|  | **6 X 2** | **12** |  |  |
| 7 | **FACINGS**1. Back & front neck facing joined (1) with straight stitchery (½)
2. Seam allowance trimmed (½) pressed open (½) and flat (½)
3. Free edge correctly edge stitched (½) and even (½)
 | 1½ 1 ½ 1 |  |  |
|  |  | **4** |  |  |
| 8 | **COLLAR PREPARATION**1. Correct shape (½)
2. Correct size (½)
3. Seam allowance layered ( ½) and snipped (½)
4. Flat collar (1)
5. Good knife edge (1)

**ATTACHING**1. Correctly attached
2. Correctly positioned
3. Straight stitchery
4. Correctly neatened with the facing
5. Trimmed (½) snipped (½)
6. Flat collar
7. Facing lying flat (1) and under stitched (1)
8. Facing fixed at the shoulder seam
 | ½ ½ 11111111121 |  |  |
|  |  | **13** |  |  |
| 9 | **FRILL PREPARATION**1. Knife pleats made (*if not award zero*)
2. Correct width of pleat
3. Pleat well pressed (½) towards the side seams (½)

**ATTACHING FRILL USING PLAIN SEAM**(If not plain seam award zero)1. Straight stitchery
2. Correct tension and size of stitches
3. Trimmed to 1cm
4. Loop stitches used (1) neat (1) evenly spaced (1)
5. $\frac{1}{3}$ of back dress neatened
 | 11111131 |  |  |
|  |  | **10** |  |  |
| 10 | **SLEEVE PREPARATION**1. Gathering evenly distributed
2. Correctly made from notch to notch
3. Correctly held and well raffled

**ATTACHING**1. Good hang
2. Notches correctly matched
3. Good stitchery (1) straight (1) correct tension (1)
4. Side seam and under arm seam meeting to within 2mm
5. Not trimmed not neatened
 | 11111311 |  |  |
|  |  | **10** |  |  |
|  | **TOTAL****DIVIDE SCORE BY 2****MARKS OUT OF 45** | **90** |  |  |