**MARKING SCHEME 441/2**

**HOME SCIENCE**

**CLOTHING AND TEXTILE**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S,NO** | **AREAS OF ASSESSMENT** | **MAX**  **SCORE** | **ACTUAL**  **SCORE** | **REMARKS** |
| 1  (a)  (b)  (c)  (d) | **PRESENTATION**  Work well pressed and folded  Label (1) firmly fixed (11/2 ) without concealing details(1) and on single (1) fabric  Pins needles (1 ½ ) and tacking threads and  Unnecessary threads removed.(1)  Left half made 1 ½ | 2 ½  2 ½  2  1 ½  1  1 ½ |  |  |
|  | **Sub total** | 11 marks |  |  |
| 2  (a)  (b)  (c)  (d)  (e) | **CUTTING OUT**  -All pieces cut out 5 interfacing(5)  - Blouses front cut smoothly (1/2) and on a straight grain  - Blouse back cut smoothly ½ and on straight grain (1 ½ )  - Pocket cut smoothly and on straight grain (1 ½ )  - Collar cut smoothly (1/2) and on  straight grain (1 1/2) | 5  ½  ½  1  ½  1 ½ |  |  |
|  | **Sub total** | 10 marks |  |  |
| 3 | **DOUBLE STITCHED SEAM SHOULDER**  If not double stitched seam award ‘O’  (a). seam made on R.S (1/2)  (b). Straight stitchery (1) on shoulder line  (c). Raw edges well tucked under ½  (d). 2nd row of stitchery don close to the fold ½ and straight ½  e). Correct width (½) 6mm (to within 2mm)  (f). Even in width (1)  (g). Seam well pressed flat (½) on R.S ½) and W.S(½) | ½  1½  1  ½  1  1½ |  |  |
|  | **Sub Total** | 7 ½ marks |  |  |
| 4 | **OPEN SEAM – SIDE SEAM**  If not open seam award ‘0’  (a). Seam jointed with straight stitchery (1 ½ )  (b). Well neatened (½) raw edges  (c). Evenness (1½) of seam allowances  i.e. 1cm to within 2mm  (e). Seam well pressed open (1) and flat on R.S (1 ½ ) and W.S(1) | 1½  ½  1 ½  ½  3 ½ |  |  |
|  | **Sub total** | 7 ½ |  |  |
| 5 | **PREPARATION AND ATTACHMENT OF THE COLLAR**  (a). Collar correctly interfaced (½)  (b). Collar pieces trimmed (½)  (c). Collar well knife edged (½)  (d). Correct size (½) and shape (½) of collar 1 1(superimposed)  (e). Collar top stitched (½) neatly and correctly  (f). Facing well edge stitched (½)  (g). Collar sandwiched between garment and facing at the front (½)  (h). Smooth stitchery (½) along neckline seam on seam line 1/2  (i) Neckline seam trimmed (1 ½ layer and snipped (½)  (j). Correct positioning of collar (½) (2)  (k). Correctly pressed flat (½) and facing (½) turned to 1 W.S (½) of garment. Front finished using facing back ½ self-neatened (1)  (l) Facing flat and catch stitched (½) along shoulder ½ seam(½) |  |  |  |
|  | **Sub total 10 ½ marks** |  |  |  |
| 6 | (a). Pocket hem turned to W.S (½) and raw edges folded under (1½)  (b). Seam trimmed (1) correct width of the hem(1)  (c).Pocket hem machine top stitched (1 ½ ) straight (½)  (d). Evenness of the pocket hem (½)  (e). Correctly attached into position (½) with straight stitchery (½) close to the fold (½)  (f). Top corners well reinforce (½)  (g). Pocket edges well tucked under (½)  (h). Correct size (½) and shape (½) of pocket (superimposed) | 2  2  2  ½  1½  ½  ½  1 |  |  |
|  | **Sub total** | 10 marks |  |  |
| 7 | **HEM MANAGEMENT**  (a). Edge stitching done (½)  (b). Evenness of the hem(½)  (c). Correctly done with slip hemming (½) stiches  (d). Quality of slip hemming stiches worked (1)  (e). Hem pressed flat (1)  (f). Facing correctly managed at the hem line (machined trimmed corner snipped and pushed out knife edge)(1) | ½  ½  ½  1  1  1 |  |  |
|  | **Sub total** | 4 ½ |  |  |
| 8 | **BUTTON HOLE**  (a). Button hole cut (1) on straight grain (1)  (b). Well-made buttonhole even stitched (1)  (c). Buttonhole stiches used (1)  (d). quality of buttonhole stich (1) tension and density  (e). Edges of buttonhole well stitched (1)  (f). Correct size 2cm (½) and position (½) of buttonhole | 2  1  1  1  1  1 |  |  |
|  | **Sub total** | 07 |  |  |
| 9 | **PREPARATION AND ATTACHMENT OF THE SLEEVE**  (i). Insertion gap 1.5cm a centimeter away from sleeve seam (2)  (ii). Gathers stiches worked using machine from notch to notch(3)  (iii). Setting-in-sleeve into armhole. With smooth stitchery.(2)  (iv). Notches matching (2)  (v). Underarm seam matching side seam (1)  (vi). Well inserted elastic band (1) and well finished (1) | 2  3  2  2  1  2 |  |  |
|  | **Sub total** | 12 marks |  |  |
| 10 | **FISHBONE STITCH**  (a).Well cut size tear (1)  (b). Fishbone stitch work (2)  (c). Loops formed at ends of stitches (2)  (d). Neat stitchery (1) | 1  2  2  1 |  |  |
|  |  | 06 |  |  |
|  | **WORK MANSHIP** | 04 ½ marks |  |  |
|  | **Grand Total** | **90** |  |  |
|  | ÷2 | **45** |  |  |