**KIJISET**

**441/2--2022**

**HOMESCIENCE.**

**CLOTHING CONSTRUCTION.**

**PAPER 2**

**PRACTICAL**

**MARKING SCHEME.**

**CANDIDATE’S NAME: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ INDEX NO. \_\_\_\_\_\_\_\_\_\_\_\_\_**

**TEACHER’S NAME:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_.**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **PROCESS** | **MAX SCORE (Marks)** | **ACTUAL SCORE** | **REMARKS** |
|  | **PRESENTATION**   1. Work well pressed (1) and well folded (1) 2. Label (½) firmly fixed on a single layer (½) of fabric 3. Pins (1) tacking threads (1) and unnecessary threads (1) removed 4. Made up left half of dress (1) | 2  1  3  1 |  |  |
|  | **Sub – total** | **07** |  |  |
|  | **CUTTING OUT**   1. All pieces cut (½x10) 2. Smooth cutting of skirt front (1) and cut on straight of grain to within 1mm (1) 3. Smooth cutting of skirt back (1) and cut on straight grain to within 1mm (1) 4. Smooth cutting of the frill (1) cut on straight grain to within 1mm (1) and cut on fold (1) 5. Smooth cutting of pocket (1) on straight grain (1) 6. Front waistband cut on straight of grain (1) 7. Straight waistband cut on straight of grain (1) | 5  2  2  3  2  1  1 |  |  |
|  | **Sub – total** | **16** |  |  |
|  | **MAKING OF BACK AND FRONT DART (MARK EACH SEPARATELY X2)**   1. Straight stitching (1) tapering to a point (1) 2. Thread and well fastened (1) at the point (1) 3. Correct width of dart (1cm) to within 3mm (1) 4. Correct length of dart (7.5cm) to within 3mm well ½ pressed and flat on R.S (½) and W.S (½) 5. Fold pressed towards C.B (½) | 2  2  1  ½  1  ½ |  |  |
|  | **Sub – total (7x2)** | 14 |  |  |
|  | **PREPARATION AND ATTACHMENT OF PATCH POCKET**   1. Placed in the correct position (1) 2. Pocket box tuck correctly stitched along stitching line (1) and pressed flat (1) 3. Pocket hem done (1) 4. Pocket mouth well secured (1) 5. Pocket turnings well tacked under round (1) 6. Pocket attached with stitching close to the edge (1) with smooth curve (1) | 1  2  1  1  1  2 |  |  |
|  | **Sub – total** | **08** |  |  |
|  | **PREPARATION OF INTERFACED WAISTBANDS**   1. **Front waistband** 2. Joined with straight stiches (1) interfaced (½) and trimmed (½) 3. Overwrapped made (3.5cm) (1) trimmed (½) and snipped sharp corners (½) 4. Turnings well tacked under and neatly held (1) 5. Hemming stitches (1) used. Quality of hemming stitches (1) 6. Even width (1) of waistband and flat on R.S (½) and W.S (½) 7. **Back waistband** 8. Joined with straight stitches (1) interfaced (½) and trimmed (½) 9. Snipped sharp corner (1) 10. Turnings well tacked under (1) 11. Tacking stitches used (1) double thread (½) and a knot made (½) to seam. 12. Even width (1) of waistband and flat on R.S (½) and W.S (½) | 2  2  1  2  2  2  1  1  2  2 |  |  |
|  | **Sub – total** | **17** |  |  |
|  | **SIDE SEAM (OPEN SEAM)**  (If not open give zero)   1. Straight stitchery (1) 2. Evenness of seam width (1) 3. Correct size or width (1-1.2cm) (2) 4. Pressed open (½) and flat on R.S (½) W.S (½) 5. Correctly neatened (1) | 1  1  2  1  1 |  |  |
|  | **Sub – total** | **6** |  |  |
|  | **ATTACHING PREPARATION AND ATTACHING OF FRILL**   1. **Knife pleats on frill** 2. Well pressed pleats (1) in the convert direction (1) convert width (1) 3. Convert positioning of pleats (1) 4. Pleats lying flat (1) at the seam lie | 3  1  1 |  |  |
|  | **Sub – total** | **5** |  |  |
|  | 1. **Lapped seam (if not lapped give zero)** 2. Frill attached with overlaid seam (1) 3. Stitched 0.2cm from fold (1) quality (½) stitches 4. Straight stitchery (1) 5. Attached with skirt seam lapping on frill (½) 6. Evenness of seam allowance (1) 7. Convert seam width, trimmed to 1cm. (1) 8. Raw edges neatened (½) correctly (½) to only half (1) 9. Quality of neatening stiches (1) 10. Seam pressed on R.S (½) and W.S (½) | **1**  **1½**  **1**  **½**  **1**  **1**  **2**  **1**  **1** |  |  |
|  | **Sub – total** | **10** |  |  |
|  | **MAKING OF BUTTON HOLE**   1. Buttonhole slashed along straight grain (½) 2. Buttonhole stitches (½) used 3. Quality of stitches (1) 4. Correct size of buttonhole (1) 1cm 5. Pressed flat (½) 6. Threads well secured (½) | (½)  (½)  1  1  (½)  (½) |  |  |
|  | **Sub – total** | **4** |  |  |
|  | **ATTACHING OF BUTTON**   1. Correctly positioned (½) 2. Firmly attached (1) 3. Shank made (1) 4. Neatly secured (½) | (½)  (1)  (1)  ( ½ ) |  |  |
|  | **Sub – total** | **3** |  |  |
|  | **Grand total** | **90/2** |  |  |
|  | **Total score** | **45** |  |  |