**HOME SCIENCE PAPER 441/2 PRACTICAL MARKING SCHEME**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **AREA OF ASSESMENT** | **MAXIMUM SCORE** | **ACTUAL SCORE** | **REMARKS** |
| 1 | **PRESENTATION** 1. Work well pressed (1) and folded (½ )
2. Label ( ½ ) firmly Fixed (1) without concealing details ( ½ ) and on single fabric ( ½ )
3. Pins /needles tacking thread and unnecessary thread removed
4. Made up for the Left half (1)
 | 1 ½ 2 ½ 1 ½ 1 |  |  |
| **SUB- TOTAL** | **6 ½**  |  |  |
| 2 | **CUTTING OUT**1. All 8 pieces
2. Smooth cutting of front Bodice (1) and on straight grain (1) to within 3mm
3. Smooth cutting of Bodice Back (1) and on straight grain. ( 1 ) to within 3mm
4. Sleeve cut on straight grain (1) and smoothly cut (1)
5. Smooth cutting (1) of collar (1) and cut on straight grain
6. Smooth cutting (1) of sleeve cuff and one grain (1)
7. Smooth cutting of neck binding
8. Smooth cutting (1) of sleeve opening strip and on grain (1)
9. Smooth cutting of interfacing
 | 822222121 |  |  |
|  **SUB – TOTAL**  | **22** |  |  |
| 3 | **FRONT WAIST DART**1. Straight stitchery (1) tapering to the point ( ½)
2. Threads ends well fastened at the point (1)
3. Correct length of dart 7 cm to within 2mm (6.8cm – 7.2cm)
4. Correct width of darts 1.5cm to within 2mm (1.3cm – 1.7 cm )
5. Dart pressed ( ½ ) towards C. F ( ½ )
6. Flatness of dart on R.s ( ½ ) and w.s ( ½ ) no pockets formed
 | 1 ½11111 |  |  |
| **SUB-TOTAL**  | **6 ½** |  |  |
|  4 | **WORKING OF MACHINE FELL SEAM** **N.B : if not machine fell seam give zero** 1. Straight stitchery of first row (1)
2. Fell well tucked under (1) and held down with straight stitchery (1) close to the edge (1)
3. Even seam (1) and correct size (1) ( 0.4 cm – 0.8cm )
4. Flat seam at R.s ( ½ ) and w.s ( ½ )
5. Fell fixed toward the back
 | 13211 |  |  |
| **SUB-TOTAL**  | **8** |  |  |
| **5** | **FRENCH SEAM (front French seam award zero from B – H)**1. Underarm seam and side seam made before sleeve is attached
2. Straight stitchery of seam (1x2)
3. Seam well trimmed ( ½ ) x2, no threads on R.S ( ½ ) x2
4. Seam well-knifed edged ( ½ ) x2
5. Evenness of seam ( ½ ) x2
6. Correct size ( 6mm ) to within 2mm (4-8 mm ) x2
7. Seam pressed towards the back at armhole( ½)x2 and at the waste line ( ½ ) x2
8. Flatness of seam at the armhole ( ½ )x2 and at the waistline ( ½ ) x2
9. Side seam and uncle arm seam meeting to within ( 2mm)

  | 1221112 |  |  |
| **SUB TOTAL**  | **13** |  |  |
| 6 | **PREPARATION AND ATTACHMENT OF THE INTERFACED COLLAR**1. Interfacing attached to under collar
2. Proper knife edging
3. Correct shape and size
4. Collar sandwiched between neck binding and garment
5. Collar flat
6. Smooth neckline
7. CB collar level with CB of bodice
8. CF collar level with CF of bodice
 | 11111111 |  |  |
| **SUB -TOTAL** | **8** |  |  |
| 7 | **CONTNOUS STRAIGHT STRIP** **SLEEVE OPENING**1. correct opening made
2. overlapsproperly made
3. correct size of opening (as per the pattern)
4. straight and even stitchery
5. hemming stitches made on w.s
 | 11111 |  |  |
| **SUB -TOTAL**  | **5** |  |  |
| 8 |  **ATTACHMENT OF SLEEVE** 1. under arm seam matching side seam
2. sleeve hanging well
3. smooth and straight stitches all round
4. evenly distributed gathers within dots of crown
5. evenly distributed gathers within the cuff
6. arm hole seam halfway trimmed (1cm) to within 2mm (0.8cm -1.2 cm)
7. a quarter of armhole seam neatened with loop stitches ( ½ )
 | 1112211 |  |  |
|  | **SUB TOTAL** | **9** |  |  |
|  |  |  |  |  |
| 9 | **SLEEVE CUFF ATTACHMENT** 1. cuff folded correctly into half
2. straight stitchery
3. trimming of seam allowances
4. correct size 3.0 – 3.2 cm wide
5. attached well on matching fitting lines
6. correctly held with tucking stitches on w.s
7. pressed flat
 | 1111111 |  |  |
|  |  **SUB TOTAL**  | **7** |  |  |
|  | **THE MAKING OF BUTTON HOLE** a) cut along the grain  b) correct size (1.3cm)  c) Buttonhole stitches used d) Depth of stitches even  e) Buttonhole not gaping open  | 11111 |  |  |
|  | **SUB – TOTALS**  | **5** |  |  |
|  | **GRAND TOTAL**  | **90** |  |  |
|  | **FINAL MARK = ACTUAL SCORE 45** **2** |  |  |