**HOME SCIENCE**

**441/2**

**PAPER 2**

**PRACTICAL**

**TIME: 2 ½ Hours**

**CEKENAS END OF TERM TWO EXAM-2022**

***Kenya Certificate of Secondary Education. (K.C.S.E)***

**FORM FOUR END OF TERM TWO EVALUATION EXAM**

**HOME SCIENCE PAPER TWO**

**CLOTHING AND CONSTRUCTION**

**MARKING SCHEME**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | PROCEDURE | MAXIMUM SCORE | ACTULA SCORE | REMARKS |
| 1 | **PRESENTATION**-Work well pressed (1) well folded(1)-label ( ½ ) firmly stitched (1) on a single fabric**½** -Pin ( ½ ) tacking threads ( ½) and unnecessary thread removed ½ Made up left half | 221 ½ 1 |  |  |
|  | **Sub - Total** | **6 ½**  |  |  |
| 2 | - **CUTTING OUT** -All pieces cut (5 x ½ )-Smooth cutting of dress CB (1) and on straight grain to within 2mm (1) | 2 ½ 2 |  |  |
|  | -Smooth cutting of sleeve (1) and on straight grain to within 2mm (1)- Smooth cutting of dress CF (1) and on straight grain to within 2mm (1)- Smooth cutting of the front neck facing (1) and on straight grain to within 2mm (1)- Smooth cutting of the back neck facing (1) and on straight grain to within 2mm ( ½ ) | 2111 1 1**½**  |  |  |
|  | Sub Total | 11 ½  |  |  |
| (a) | **FRENCH SEAM****The making of a French seam at the shoulder [If not French seam award a zero]**-Straight stitching (1)-Correct width 5.8 – 6.2 mm (1)-Raw edges (1) and thread concealed ( ½ )-Pressed (1) towards C.B (1) -Good knit edge (1) -Seam made on W.S (1) | 111 ½ 211 |  |  |
|  | Sub - Total | 7 ½  |  |  |
| (b) |  **Making of the side seam using neatened plain seam.( If not plain seam give a zero)**-Straight stitchingCorrect width 0.8 – 1.2 cm ( to within 2mm)-Correct neatened using loop stitches (1)- Overcasting stiches even length and tension ( ½ ) and even depth ( ½)-Seam allowance even-Straight even edges-Seam made on W.S | 1112211 |  |  |
|  | Sub Total  | 9 |  |  |
| ( c)  | **Joining of the underarm seam using a neatened open seam ( if not open give zero)** -Correct seam (1)-Evenness in width (1)-Straight stitchery (1)-Flat open(1)-Well neatened using edge stitching-Straight edges-Pressed open -Underarm seam meeting with side seam-Made on the W .S | 111121111 |  |  |
|  | **Sub-Total** | 10 |  |  |
| (d) | -**Attaching of lace on the lower edge of the sleeve** **using an overlaid seam ( if not overlaid give a zero)**-Lace folded ( ½ ) on the seam line (1)-Lace placed on the fitting line lower sleeve (1)-Straight stitchery (1) at the edge of the fold to within 2mm (1)-Seam allowance 1.5 from fitting line to within 2mm 1.3 – 1.7cm (1)-Flatness of lace on 12.5 (1)-Overlaid seam turning facing up ( ½ ) and even ½  | ( 1 ½ )12111 |  |  |
|  | **Sub-Total** | 7 ½  |  |  |
| (e) | **Preparation and attachment of the sleeve** -Correctly prepared (2)-Gathers evenly distributed (1)-Sleeve set correctly-Straight and smooth stitchery (1) on the armhole (2)-Under ram seam and side seam meeting (1)-Evenness in width-Armhole neatened with loop stitch ( if it loop award zero) loop stitches evenly spaced (1) and even in the length- Seam evenly trimmed (1) and stitches secured / fastened on (1) and off (1) | 21121123 |  |  |
|  | **Sub-Total** | 13 |  |  |
| (f) | -**Preparation and attachment of neck facing**-Back (1) and front(1) facing correctly joined-Free edge of the facing edge stich neatly (1)-An even edge throughout (1)-Seam evenly trimmed (1) open (1) and lying flat(1)-Facing correctly and with straight stitchery (1) and edge wall rounded and smooth (2)-Facing lying flat (1)-Seam allowanced trimmed (1) and clipped (1)Facing under stitched (1) | 2114121 |  |  |
|  | **Sub-Total** | 17 |  |  |
| (g) | **Management of the dress hem** -Correct hemming stitches (2)-Even and neat stiches (1)-Raw edges neatened (1) and folded on the hem line (1)Hem hand made-Stitches not too conspicuous on the R.S (1) | 211211 |  |  |
|  | **Sub-Total** | 8 |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **GRAND TOTAL** | $\frac{90}{2}$ =45 |  |  |