**441/2**

**HOME SCIENCE**

**(CLOTHING CONSTRUCTION)**

**PAPER 2**

**JUNE/JULY 2021**

**MOKASA 1 J O I N T E X A M I N A T I O N**

**JUNE/JULY 2021**

**441/2**

**HOME SCIENCE**

**CLOTHING AND CONSTRUCTION**

**PAPER 2**

**MARKING SCHEME**

**Candidates Name: …………………………………………………………………………..**

**Index No.: ………………………………………**

**Subject Teacher’s Name: …………………………………………………………………**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  | **TASKS** | **MAX. SCORE**  | **ACTUAL SCORE** | **REMARKS** |
| **1.** |  | **PRESENTATION** |  |  |  |
|  | (a) | Work well ironed and folded | 1 |  |  |
|  | (b) | Work well labelled with clearly written name; Adm. No. and class. | 1 ½  |  |  |
|  | (c) | Label firmly sewn on a single fabric without concealing details. | 1 ½  |  |  |
|  | (d) | Pins, needles and unnecessary hanging threads removed. | 1 |  |  |
|  | (e) | Made the right half of the dress  | 1 |  |  |
|  |  | **SUB TOTAL** | **6**  |  |  |
|  |  |  |  |  |  |
| **2.** |  | **CUTTING OUT** |  |  |  |
|  | (a) | Cutting out. | 4 |  |  |
|  | (b) | Front dress cut smoothly and as straight grain. | 2 |  |  |
|  | (c) | Back dress cut smoothly and on straight grain. | 2 |  |  |
|  | (d) | Yoke cut smoothly and on straight grain. | 2 |  |  |
|  |  | **SUB TOTAL** | **10** |  |  |
|  |  |  |  |  |  |
| **3.** |  | **DOUBLE POINTED DART** |  |  |  |
|  | (a) | Straight firmly and straightly | 1 |  |  |
|  | (b) | Tapening to nothing on both ends and without pockets. | 2  |  |  |
|  | (c) | Well reignforced on both ends. | 2 |  |  |
|  | (d) | Slashed at the centre and well neatened. | 2 |  |  |
|  | (e) | Correct size (Length and width) | 2 |  |  |
|  | (f) | Well pressed and flat. | 1 |  |  |
|  |  | **SUB TOTAL** | **10** |  |  |
|  |  |  |  |  |  |
| **4.** |  | **POCKET** |  |  |  |
|  | **I.** | **Working of satin stitches** |  |  |  |
|  | (a) | Satin stitches worked. If not give zero the whole section. | 1 |  |  |
|  | (b) | Correct tension. | 1 |  |  |
|  | (c) | Evenness of the stitches | 1 |  |  |
|  | (d) | Neatness of the stitches | 1 |  |  |
|  | (e) | The oval shape well filled (No gaps). (Mark by impression). | 1 |  |  |
|  | (f) | Well reinforced on and off | 2 |  |  |
|  |  | **SUB TOTAL** | **7** |  |  |
|  |  |  |  |  |  |
|  | **II** | **Preparation and attachment** |  |  |  |
|  | (a) | Pocket hem with two turnings to conceal the raw edge. | 1/2 |  |  |
|  | (b) | Hem stitched in position close to the fold with firm and straight stitchery. | 1 ½  |  |  |
|  | (c) | Sides and bottom of the pocket well folded to the W.S and trimmed to 0.5cm (to within 2mm) | 3  |  |  |
|  | (d) | Bottom corners mitred. | 2 |  |  |
|  | (e) | Pocket attached with firm; straight stitches close to the fold. | 3 |  |  |
|  | (f) | Pocket opening reinforced on both sides. | 2 |  |  |
|  | (g) | Correct size of the pocket | 1 |  |  |
|  | (h) | Correct shape of the pocket | 1 |  |  |
|  | (i) | Correct positioning of the pocket | 1 |  |  |
|  | (j) | Pocket placed rightly (not upside down) | 1 |  |  |
|  | (k) | Pocket pressed flat | 1 |  |  |
|  |  | **SUB TOTAL** | **17** |  |  |
|  |  |  |  |  |  |
| **5.** | **I.** | **Working of gathers on the front dress** |  |  |  |
|  | (a) | Gathers made on the marked part of the dress. | 1 |  |  |
|  | (b) | Made gathers and not pleats. | 1 |  |  |
|  | (c) | Gathers evenly distributed | 1 |  |  |
|  | (d) | Gathering stitches made 0.6cm above and below the stitching line. | 2 |  |  |
|  |  | **SUB TOTAL** | **5** |  |  |
|  |  |  |  |  |  |
|  | **II.** | **Working overlaid seam on the yoke and front dress (If not overlaid give zero)** |  |  |  |
|  | (a) | Yoke folded to W.S on the stitching line. | 1 |  |  |
|  | (b) | Placed on the R.S. of the front dress at the stitching line.  | 1 |  |  |
|  | (c) | Seam done with straight and firm stitchery and close to the fold. | 1 ½  |  |  |
|  | (d) | Seam turnings trimmed to 1 cm | 1  |  |  |
|  | (e) | Seam turnings neatened together. | 1 |  |  |
|  | (f) | Appropriate neatening stitches *(If not give zero from f – j)* | 1 |  |  |
|  | (g) | Evennes of stitches | 1 |  |  |
|  | (h) | Good tension | 1 |  |  |
|  | (i) | Fastened on and off | 2 |  |  |
|  |  | **SUB-TOTAL** | **10 ½**  |  |  |
| **6.** |  | **Shoulder seam (Double stitched seam)****(If not give zero)** |  |  |  |
|  | (a) | Straight and firm stitchery of the first line | 1 |  |  |
|  | (b) | Straight and firm stitchery of the second line and close to the fold.  | 1 ½ |  |  |
|  | (c) | Seam neatly tucked to conceal the raw edges | 1 |  |  |
|  | (d) | Correct size of the seam 6mm to within 2mm  | 1 |  |  |
|  | (e) | Fell folded to the back | 1 |  |  |
|  | (f) | Flat on the W.S and R.S | 1 |  |  |
|  | (g) | Evenness of he complete seam | 1 |  |  |
|  |  | **SUB TOTAL** | **7 ½**  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
| **7.** |  | **Side seam (Open seam) *If not give zero*** |  |  |  |
|  | (a) | Seam done with firm and straight stitchery. | 1 |  |  |
|  | (b) | Seam turnings neatened separately and appropriately. | 2 |  |  |
|  | (c) | Correct size of the neatened seam 1cm to within 2mm  | 1 |  |  |
|  | (d) | Evenness of the neatened turnings turning | 1 |  |  |
|  | (e) | Seam pressed open and flat at the hem.  | 2 |  |  |
|  |  | **SUB TOTAL** | **7** |  |  |
|  |  |  |  |  |  |
| **8.** |  | **Hem Management** |  |  |  |
|  | (a) | A narrow turning done to conceal the raw edge. | 1 |  |  |
|  | (b) | A second turning made at the foldline. | 1 |  |  |
|  | (c) | Hem held with even tacking. | 1 |  |  |
|  | (d) | Held using hemming stitches. *If not give zero from d-g*. | 1 |  |  |
|  | (e) | Evenness of the stitches used. | 1 |  |  |
|  | (f) | Good tension used | 1 |  |  |
|  | (g) | Fastened on and off. | 1 |  |  |
|  | (h) | Correct size of the hem 1.5cm to within 2mm | 1 |  |  |
|  | (i) | Evenness of the hem. | 1 |  |  |
|  | (j) | Flatness of the hem | 1 |  |  |
|  |  | **SUB TOTAL** | **10** |  |  |
|  |  | **GRAND TOTAL** | **90/2** |  |  |