**441/2**

**HOMESCIENCE PAPER 2**

**FORM 4**

**MID TERM II 2020**

***MERU CENTRAL CLUSTER EXAMINATION***

***KENYA CERTIFICATE OF SECONDARY EDUCATION (KCSE)***

**Marking Scheme**

|  |  |  |
| --- | --- | --- |
|  | **PRESENTATION*** Work well pressed ½ and folded ½
* Lebel (1) firmly fixed ½ on a single fabric ½ without concealing details
* Pins and needles removed ½
* Tacking ½ and unnecessary hanging ½ threads removed
* Made up for the left side (1)
 | 1**2**111 |
|  | **Sub Total** | **6** |
|  | **CUTTING OUT*** All six pieces cut out ( ½ x 6)
* Cutting of front bodice straight (2) and cut on grain (1) to within 2 mm
* Cutting of back bodice straight (2) and cut on grain (1)
* Back skirt cut straight (1)
* Front skirt cut straight (1)
* Smooth cutting of colar (1) and on straight grain (1) to within 2mm
* Smooth cutting of the lower edge of the skirt( 2 ) front and back

( 2 )* Neck binding cut out on bias (1)
 | 33311241 |
|  | **Sub Total** | **18** |
|  | **THE DART*** Dart made with straight stitchery (1)
* Dart tapering ½ and fastened ½ at the point
* Correct length of dart (1) to within 2mm(72cm – 7.6cm)
* Correct width of dart (1) (mark at the seam)to within 2mm(1.2cm -1.6cm)
* Flatness of dart on W.S ½ and R.S. ½
* Dart pressed towards the C.F ½
 | 111111( ½) |
|  | **Sub Total** | **6½**  |
|  | **SEAM (OPEN SEAM)**(if not seam give 0)* Seam attached with straight stitchery (2)
* Seam appropriately neatened (2 x 2)
* Evenness of the neatened seam 2
* Correct size of seam 1 cm to within 2mm ( 0.8 – 1.2 cm) (2 x 2)
* Seam open ( ½ ) and flat on R.S ( ½)and W.S (½ )
 | **2****4****2****4****1½**  |
|  | **Sub Total** | **13 ½**  |
|  | **SIDE SEAM (BODICE AND SKIRT) FRENCH SEAM**(If not French award 0)* 1st line of stitching straight (1) (mark by impression) 1 x 2
* 2nd line of stitching done on the seam line (2) 1 x 2
* Evenness of the seam (2) 2 x 2
* Raw edges well concealed on the R.S (1) 1 x 2
* Correct size (width to within 2mm) (2)(0.4 – 0.8cm) 2 x 2
* Seam well knife edged (2) 2 x 2
* Flat at waist (1) 1 x 2
* Pressed towards back (at the waist) 1 x 2
 | **2****2****4****2****4****4****2****2** |
|  | **Sub Total** | **22** |
|   | **OVERLAID SEAM*** Straight stitchery (2) 1 x 2 close to the fold (1) 1 x 2
* Seams matching where they cross(i.e side seam of bodice and skirt) (1)
* Half seam neatened (1)
* Overcasting stitches done well (1)
* Correct width of seam (1) (0.4 – 0.8cm)
 | **4****1****1****1****2** |
|  | **Sub Total** | **9** |
|  | **PREPARATION OF THE COLLOLAR AND ATTACHMENT*** Good stitchery along the seam allowance (1)
* Seam allowance trimmed to within 1mm to avoid bulk (1)
* Knife edged all round (1) curves well rounded (1)
* Correctly positioned 1
* Flatness of the attached collar 1
* Cross way strip even(1) and appropriately worked/hemmed (1)
* Correct shape 1 and size(1) of the attached collar(super impose)
* Neckline seam evenly trimmed (1) and snipped (1)
* Collar attached by sandwiching between the dress ½ and cross way strip ½
 | **1****1****2****1****1****2****2****2****1** |
|  | **Sub Total** | **13**  |
|  | **EDGE STITCHING THE HEM*** Straight stitchery (1)
* Even edge (1)
 | **1****1** |
|  | **Sub Total**  | **2** |
|  | **Grand Total** | **90** |